	COSHH Assessment
Hollins & Reed Contracting Ltd



	Project or site
House refurbishment, House 7
	Assessment ref
CA-004
	Date assessed
5 October 2026



	Substance
	
	
	

	Product or substance
	Hypochlorite cleaner, about 5%
	Supplier
	your supplier

	SDS date
	your sheet’s date
	Form (liquid, dust…)
	Liquid



	The work
	
	
	

	Task
	Cleaning toilet and cabin
	Where
	Welfare cabin

	How often, how long
	Daily, 20 minutes
	Amount, used with
	Up to 500 ml, no other cleaners



	Hazards (H codes)
	Harmful or irritant
	Corrosive
	Toxic
	Serious health hazard
	Cancer or asthma
	Flammable

	H314, H318, H410.
	☒
	☒
	☐
	☐
	☐
	☐



	How it gets in
	Breathing in
	Skin
	Eyes
	Swallowing
	Puncture

	Splashes, gas if mixed
	☒
	☒
	☒
	☐
	☐



	Who could be harmed
	People doing it
	Others nearby
	Cleaners, fitters
	Visitors, public
	Higher risk

	Cleaner, others in the cabin
	☒
	☒
	☐
	☐
	☐



	Health effects

	Burns skin and damages eyes. Weaker solutions still irritate. Very toxic to water life.

	EUH031: with acid cleaners it gives off toxic chlorine gas. Hands wet over 2 hours a shift can cause dermatitis.



	Controls
	In place
	Still needed

	Avoid or swap it
	Detergent first. Bleach only where needed.
	

	Change the method
	As bought, or into water. Add nothing else.
	

	Extract at source
	Door and windows open while cleaning.
	

	Fewer, for less time
	One named person. Smallest bottle, kept shut.
	

	Washing, welfare
	Warm water, soap and towels at the cabin.
	



	PPE: type or standard
	Gloves
	Eye protection
	RPE
	Overalls
	Boots

	EN 374 gloves. Goggles if pouring.
	☒
	☒
	☐
	☐
	☐



	If it goes wrong
	

	Spill or leak
	Ventilate, dilute with plenty of water, mop up. Not down a surface drain.

	Fire
	Does not burn. If there is a fire nearby, leave and call 999.

	First aid
	Skin: flood 20 minutes. Eyes: at least 10 minutes, hospital. Swallowed: rinse mouth, 999.



	Further action
	Who
	By when
	Checked

	Move acid toilet cleaner to a separate shelf
	DH
	Before start
	



	Assessed by
Dan Hollins
	Signed

	Date
5 October 2026
	Next review
5 October 2027



Worked example. Typical product. Your supplier’s safety data sheet governs.
