	COSHH Task Assessment
Hollins & Reed Contracting Ltd



	Project or site
Basement fit-out, Block B
	
	Trade
Groundworks
	
	Date assessed
5 October 2026
	
	Assessment ref
CA-013



	What the work makes
	
	
	

	Task
	Running plant
	Material worked
	Diesel engines

	Dust or fume made
	Diesel engine exhaust
	Tool used
	Generator, 1 tonne dumper

	Where
	Partly enclosed basement
	How long a shift
	Dumper up to 2 hours a day



	Exposure limit
	
	
	

	WEL, 8-hour
	None for exhaust. CO 20, NO2 0.5 ppm
	WEL, 15-minute
	CO 100, NO2 1 ppm

	Monitoring result
	CO2 640 ppm, an indicator
	Measured on
	2 October 2026



	Who could be harmed
	People doing it
	Others nearby
	Cleaners, fitters
	Visitors, public
	Higher risk

	Driver, everyone in the basement
	☒
	☒
	☐
	☐
	☐



	Health effects

	Irritates eyes and airways. Long exposure, above all to blue or black smoke, can cause coughing and breathlessness.

	Repeated exposure over many years can increase the risk of lung cancer.



	Controls
	In place
	Still needed

	Another method
	Generator outside, exhaust away from the fan.
	Price an electric dumper.

	On-tool extraction
	Not used on the dumper.
	

	Water suppression
	Not used on exhaust.
	

	Room ventilation
	Fan blows fresh air in. Ramp doors open.
	

	Fewer, for less time
	Engine off when idle. One dumper down at a time.
	

	Clean-up
	Soot on walls means control is failing: stop.
	



	RPE: type and filter
	Disposable
	Half mask
	Powered
	Face-fit tested
	Eye protection

	Not used. RPE is the last resort.
	☐
	☐
	☐
	☐
	☐



	Also needed
	Yes
	No
	Detail
	Next due

	Exposure monitoring
	☒
	☐
	CO2 meter. Over 1000 ppm: stop, check fan.
	Weekly

	Health surveillance
	☐
	☒
	None required for exhaust. Irritation: stop.
	

	LEV examination
	☐
	☒
	None used.
	

	Training
	☒
	☐
	Smoke colours, engine off, fan, soot.
	Before start



	Further action
	Who
	By when
	Checked

	Dumper serviced, no blue or black smoke
	DH
	Before start
	

	Fan and CO2 meter on site
	DH
	Before start
	



	Assessed by
Dan Hollins
	
	Signed

	
	Date
5 October 2026
	
	Next review
5 October 2027



Worked example. Change it to fit your job before you use it.
