	COSHH Assessment
Hollins & Reed Contracting Ltd



	Project or site
House refurbishment, House 7
	Assessment ref
CA-002
	Date assessed
5 October 2026



	Substance
	
	
	

	Product or substance
	Petrol (unleaded)
	Supplier
	your supplier

	SDS date
	your sheet’s date
	Form (liquid, dust…)
	Liquid and vapour



	The work
	
	
	

	Task
	Refuelling saw and generator
	Where
	Outdoors, marked refuelling spot

	How often, how long
	Daily, under 5 minutes each
	Amount, used with
	Up to 5 litres, nothing mixed in



	Hazards (H codes)
	Harmful or irritant
	Corrosive
	Toxic
	Serious health hazard
	Cancer or asthma
	Flammable

	H304, H340, H350.
	☐
	☐
	☐
	☒
	☒
	☒



	How it gets in
	Breathing in
	Skin
	Eyes
	Swallowing
	Puncture

	Vapour, splashes, siphoning
	☒
	☒
	☒
	☒
	☐



	Who could be harmed
	People doing it
	Others nearby
	Cleaners, fitters
	Visitors, public
	Higher risk

	Refueller, anyone nearby
	☒
	☒
	☐
	☐
	☐



	Health effects

	May cause cancer and genetic defects. May be fatal if swallowed and enters the airways. Flammable: code on your sheet.

	Treat as a carcinogen: petrol contains benzene. No EH40 limit for petrol; benzene 1 ppm over 8 hours.



	Controls
	In place
	Still needed

	Avoid or swap it
	Battery or mains tools where the job allows.
	Price a battery cut-off saw.

	Change the method
	Engine off, cool. Spout. No smoking or flames.
	Extinguisher at the spot.

	Extract at source
	Open air only. Not in a van, cabin or trench.
	

	Fewer, for less time
	One trained person. UN-approved cans, shut.
	Cans in a ventilated lock-up.

	Washing, welfare
	Wash splashes off. Change splashed clothes.
	



	PPE: type or standard
	Gloves
	Eye protection
	RPE
	Overalls
	Boots

	Gloves per sheet, safety glasses.
	☒
	☒
	☐
	☐
	☐



	If it goes wrong
	

	Spill or leak
	Stop engines and flames. Spill kit, keep out of drains, bag as hazardous waste.

	Fire
	Clear the area, call 999. Extinguisher only if trained and it is safe.

	First aid
	Swallowed: do not make them sick, 999. Eyes: flush at least 10 minutes, then hospital.



	Further action
	Who
	By when
	Checked

	Extinguisher, lock-up and DSEAR assessment done
	DH
	Before start
	



	Assessed by
Dan Hollins
	Signed

	Date
5 October 2026
	Next review
5 October 2027



Worked example. Typical product. Your supplier’s safety data sheet governs.
