	COSHH Task Assessment
Hollins & Reed Contracting Ltd



	Project or site
House refurbishment, House 7
	
	Trade
Drylining
	
	Date assessed
5 October 2026
	
	Assessment ref
CA-011



	What the work makes
	
	
	

	Task
	Cutting, sanding joints
	Material worked
	Plasterboard, jointing compound

	Dust or fume made
	Gypsum dust, inhalable
	Tool used
	Handsaw, rasp, pole sander

	Where
	Indoors, one room at a time
	How long a shift
	About 3 hours



	Exposure limit
	
	
	

	WEL, 8-hour
	Gypsum 10 mg/m³, respirable 4
	WEL, 15-minute
	None listed

	Monitoring result
	Not measured
	Measured on
	Not measured



	Who could be harmed
	People doing it
	Others nearby
	Cleaners, fitters
	Visitors, public
	Higher risk

	Dryliner, others, cleaner
	☒
	☒
	☒
	☐
	☐



	Health effects

	Breathing a lot of dust can damage the lungs and airways. Gypsum has very little silica, but board dust can carry some.

	Jointing compound and plasters may hold quartz: read their sheet.



	Controls
	In place
	Still needed

	Another method
	Tapered-edge boards. Handsaw and rasp, not a power saw.
	

	On-tool extraction
	Pole sander on an M class unit.
	

	Water suppression
	Not used on board.
	

	Room ventilation
	Window open, door shut to other rooms.
	

	Fewer, for less time
	Only the dryliner in the room while sanding.
	

	Clean-up
	Class M vacuum. No dry sweeping.
	



	RPE: type and filter
	Disposable
	Half mask
	Powered
	Face-fit tested
	Eye protection

	APF 20 for sanding: disposable FFP3.
	☒
	☐
	☐
	☒
	☐



	Also needed
	Yes
	No
	Detail
	Next due

	Exposure monitoring
	☐
	☒
	Extraction checked daily. Dust escaping: stop.
	

	Health surveillance
	☐
	☒
	Only if a cough or wheeze is reported.
	

	LEV examination
	☒
	☐
	Examined at least every 14 months.
	March 2027

	Training
	☒
	☐
	Extraction, clean shaven, clean-up.
	Before start



	Further action
	Who
	By when
	Checked

	Sander and M class unit on site
	DH
	Before start
	



	Assessed by
Dan Hollins
	
	Signed

	
	Date
5 October 2026
	
	Next review
5 October 2027



Worked example. Change it to fit your job before you use it.
