	Working at Height Permit
Hollins & Reed Contracting Ltd



	Permit no.
HR-0422
	Site
Unit 5, Canal Side Business Park
	Exact location
Flat roof, south section, inside the barrier



	Details
	
	
	
	
	

	Contractor
	Hollins & Reed
	Issued to
	Owen Tattersall
	Valid from
	22/10/26 07:45

	Valid to
	22/10/26 12:30
	RAMS ref
	HR-RAMS-12
	
	



	The work
	

	Where and how reached
	Large felt roof, concrete deck. Fixed ladder to a hatch inside the barrier, 9 m from the edge.

	Work to be done
	Set the barrier. Two-hour condition survey, photos and moisture readings. Strike the barrier.

	Why not from ground
	Pole camera pictures on 15 October could not show if the felt is wet. That needs a meter.



	Hazards
	
	
	
	
	
	
	

	Fragile roof
	☒
	Unprotected edge
	☒
	Roof lights
	☒
	Weather
	☒

	Overhead lines
	☐
	People below
	☒
	Lone working
	☐
	Falling objects
	☒



	Precautions
	Done
	By

	Access equipment inspected
	☒
	Dan Hollins

	Edge protection in place
	☐
	Barrier 2 m instead

	Fragile surfaces covered or barriered
	☒
	Barrier, by 08:50

	Harness and anchor points
	☐
	Not needed. No anchor

	Rescue plan in place
	☒
	See below

	Exclusion zone below
	☒
	Keyholder, cones

	Weather checked
	☒
	Readings, sheet 2

	Tools tethered
	☒
	Wrist straps

	Lighting
	☐
	Not needed. Daylight



	Equipment
	
	
	
	
	
	
	

	MEWP
	☐
	Tower
	☐
	Scaffold
	☐
	Harness
	☐

	Netting
	☐
	
	☐
	
	☐
	
	☐



	People on this permit: name
	Company
	Briefed

	Owen Tattersall, Joe Penketh: survey
	Hollins & Reed
	☒

	Reece Ollerton, Priya Shah: barrier
	Hollins & Reed
	☒



	Other conditions

	Issuer at the hatch while anyone works. Stay inside the barrier. Stop at a steady 8 m/s, our limit for this job, or on rain.

	Rescue: no harness. Hurt or ill: ring 999, say fixed ladder, may need fire service. Issuer meets them at the hatch.



	Sign-off
	Name
	Signature
	Date
	Time

	Issued: precautions checked
	Dan Hollins
	signed
	22/10/26
	07:35

	Accepted: permit understood
	Owen Tattersall
	signed
	22/10/26
	07:40
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	Weather and equipment checks

	Time
	Wind
	By
	Result

	07:30
	2.4 m/s
	Reece Ollerton
	Read at the hatch, before issue. Dry. Under our limit.

	07:45
	2.6 m/s
	Reece Ollerton
	All four briefed by the issuer. Barrier team up. Our method for this job: sections and weights hauled through the hatch on a rope, nobody on the ladder while a load moves. Line taped out from the hatch first, sections set from inside it, one setting, one watching. Nobody past the tape.

	08:50
	2.9 m/s
	Dan Hollins
	Barrier done, weighted, 2 m from edges and roof lights. Team stopped while the issuer walked it. Team down.

	09:00
	3.1 m/s
	Joe Penketh
	Survey team up. Dry. Under our limit.

	10:00
	4.4 m/s
	Joe Penketh
	Dry. Both inside the barrier. Issuer at the hatch.

	11:00
	6.3 m/s
	Joe Penketh
	Wind rising, cloud building. Last readings, then off the roof.

	11:20
	6.6 m/s
	Reece Ollerton
	Under our limit. Barrier team up. Sections lifted back towards the hatch, nobody past the line. Issuer at the hatch.

	11:55
	7.1 m/s
	Reece Ollerton
	Last section lowered through the hatch. Team down.

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	Cancellation
	

	Work stopped at
	11:55. Survey done 11:10, barrier struck 11:55. All four down and counted.

	Area left safe
	Hatch shut and locked 12:00. Nothing left on the roof.

	Equipment removed
	Barrier sections to the van. Cones lifted 12:05.



	Handback
	

	Area returned to
	Thornley Vale Estates Ltd, site keyholder, 12:15

	Notes
	Survey report to follow. Not part of this permit.



	Sign-off
	Name
	Signature
	Date
	Time

	Extended: new end time
	Not extended
	
	
	

	Cancelled: area checked
	Dan Hollins
	signed
	22/10/26
	12:10

	Handed back: area returned
	Dan Hollins
	signed
	22/10/26
	12:15



Worked example of a made-up job. Not a permit.   ·   Page 1 of 1
